ATIFLASH.EXE
============
[3.60]
  - Use SCLK to flash BIOS on RV730 only (SCLK will be scaled down while flashing the BIOS)

[3.59]
  - Add RV730 support

[3.58]
  - fix pa paramter, synchornize the same behaviour as ATIWinFlash

[3.57]
  - Add R700 Support
  - Reduce size

[3.56]
  - fix corrupted zip file. Same releaes as 3.55

[3.55]
  - add option (excl_memtrain_dtable) to keep memory training information while flashing new bios
  - add partial check for -pavbpn

[3.54]
  - Add "nw" in help 

[3.53]
  - Add unique identifier for Ry7xx

[3.52]
  - Add RV770 device ID support

[3.51]
  - add -AMD flag to allow searching for devices with AMD vendor ID

[3.50]
  - update SPI write sequence to check for both WREN and BUSY bits to be deasserted before verifying the     write (solves issues seen with intermittent write failures)

[3.49]
  - update description for RV670 slave devices to identify uniquely on Gemini boards

[3.48]
  - correctly print Old and New P/N when flashing with newer bioses

[3.47]
  - explicitly identify RV635 ASICs

[3.46]
  - fix problems with GPIO19 asserting the CTF signal on RV670 boards

[3.45]
  - fix problems with crashes on some systems when flashing onto blank ROMs

[3.43]
  - added -pavbpn (allows the use of -pa with VBIOS PN)
  - added support for new ROM used by multimedia cards (Quito and Lima)

[3.42]
  - fix -mb command for Ry6xx

[3.41]
  - fix Ry6xx SST support

[3.40]
  - fix RV610 + Rialto hang issue

[3.39]
  - fix RV610 write issue

[3.38]
  - Add Quito support

[3.35]
  - resolved -i/-ai corruption issue

[3.34]
  - -ai now displays full PCI ID information
  - ATMEL flash procedurce redesigned for stability/reduced overall flash time
  - -ai -scansii combination will report SST/ATMEL firmware revision

[3.33]
  - internal release

[3.32]

  -add flashing over 128KB

[3.31]

  -resolved pak issues with SST/ATMEL

[3.30]

  -update device ID support for RV630/M76 & 0x000 for Ry6xx

[3.29]

  -add new option -pak to build flash package

[3.28] 11/02/06

  -add new option -fa to force flashing if the ROM is already programmed
  -add new option -fm to force flashing if legacy memory config mismatch
  -add new option -fs to force flashing if SSID mismatch
  -add new option -fp to force flashing if BIOS P/N mismatch
  -add new command -pa to search and program multiple adapters according to
   BIOS P/N
  -add new option -padevid to search for adapters of a specific PCI device
   ID when used with -pa command
  -add new option -passid to search for adapters of a specific subsystem
   ID when used with -pa command
  -add new option -pasvid to search for adapters of a specific subsystem
   vendor ID when used with -pa command


Older revisions
=============================

[3.00]  09/08/04

  - initial release

[3.01]  09/16/04

  - adjust bus scanning sequence

[3.02]  09/30/04

  - add Rialto support

[3.03]  10/19/04

  - fix issues for Rialto

[3.04]  12/01/04

  - remove 32K limit for Rialto

[3.05]  12/09/04

  - add RN50 support

[3.06]  03/03/05

  - fix issue in flashing secondary adapters

[3.07]  03/15/05

  - fix SST support with -sst option
  - fix infinite looping on write failure

[3.08]  04/05/05

  - display BIOS P/N in -i option

[3.09]  04/29/05

  - add -mi command to modify SSID in ROM image
  - add support R530

[3.10]  09/30/05

  - support write-protected sector on 128k serial flash ROMs
  - add RIO support
  
[3.11]  11/11/05

  - mask out GENERICD pad output register clear to avoid setting VDDC on A520xx-20 PCB

[3.12]  11/14/05

  - add verified LIMA support
  
[3.13]  02/03/06

  - add new option -mb for modifying BIOS SSID, SVID, BIOS P/N and bootup message

[3.14] 02/13/06

  - add update SiImage firmware
  
[3.15] 02/24/06
  
  - add support for Warhol (RV570/M68/RV560/M67) device IDs
  - mask out GPIO[6..3] clear to avoid overwriting MVP settings on RV570/RV560
  
[3.16] 04/24/06
  
  -allow autodetect and/or pin specification for SiImage firmware updating

[3.17] 05/23/06
  
  -fix issues with sst ROMs
  
[3.18] 05/26/06
  
  -fix SiImage Firmware update issue

[3.19] 06/02/06
  
  -improve SiImage Firmware process

[3.20] 06/09/06
  
  -Add new options, -reboot, -pci, -pcie, -agp, -noagp, -nopcie
  -Fix SiI1930 Mobile FW Update issues

[3.21]

  -add new command -ai, advanced information
  -add new options -log, -logappend
  -reformat help menu, help menu appears with use of -h, /h, -? or /?

[3.22]

  -add display more BIOS information when flashing
  -add reboot message when flashing completed successfully

[3.23]

  -fix minor message issue


[3.24]

  -Update Lima Support
  
[3.25]
 
  -Add RV550/M71 Support


